	Model 4160 
Connector, BNC (Female), Bulkhead 


[image: ]
 
FEATURES: 
•    Connector meets the interface requirements of MIL-STD-348 
 
MATERIALS: 
Body and Fittings – Brass, Tarnish Resistant Plating  
Center Contact – Gold Plated Beryllium Copper 
Dielectric: PTFE 
Marking: “Pomona 4160” 
 
RATINGS: 
Operating Voltage: Shield/Earth: 30VAC/60VDC Max. 
                              Inner Conductor/Shield: 500VRMS Max. 
Operating Temperature: -65ºC to +165ºC 
Nominal Impedance: 50 Ohms 
 
ORDERING INFORMATION: Model 4160 
Parts are packaged one per bag, unassembled. 
All dimensions are in inches. Tolerances (except noted): xx = ±.02” (,51 mm), .xxx = ± .005” (,127 mm). 
All specifications are to the latest revisions. Specifications are subject to change without notice. 
Registered trademarks are the property of their respective companies.  Made in USA 
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